CPCCCO2011A Handle concreting materials

Release: 1

CPCCCO2011A Handle concreting materials

Modification History

Not Applicable

Unit Descriptor

Unit descriptor	This unit of competency specifies the outcomes required to safely manually handle, store and apply environmental management principles associated with concreting materials and components in preparation for concreting work to commence. The unit includes the identification and safe handling of hazardous materials and waste in accordance with material safety data sheets (MSDS).

Application of the Unit

Application of the unit	This unit of competency supports the attainment of the understanding and skills to correctly and sustainably handle concreting materials, which may include working with others and as a member of a team.

Licensing/Regulatory Information

Not Applicable

Pre-Requisites

Prerequisite units
CPCCOHS2001A	Apply OHS requirements, policies and procedures in the construction industry

Employability Skills Information

Employability skills	This unit contains employability skills.

Elements and Performance Criteria Pre-Content

Elements describe the essential outcomes of a unit of competency.	Performance criteria describe the performance needed to demonstrate achievement of the element. Where bold italicised text is used, further information is detailed in the required skills and knowledge section and the range statement. Assessment of performance is to be consistent with the evidence guide.

Elements and Performance Criteria

ELEMENT	PERFORMANCE CRITERIA
1. Plan and prepare.	1.1. Work instructions and operational details are obtained using relevant information, confirmed and applied for planning and preparation purposes. 1.2. Safety (OHS) requirements are followed in accordance with safety plans and policies. 1.3. Signage and barricade requirements are identified and implemented. 1.4. Tools and equipment selected to carry out tasks are consistent with the requirements of the job, checked for serviceability and any faults are rectified or reported prior to commencement. 1.5. Materials quantity requirements are calculated in accordance with plans, specifications and quality requirements. 1.6. Materials appropriate to the work application are identified, obtained, prepared, safely handled and located ready for use. 1.7. Environmental requirements are identified for the project in accordance with environmental plans and regulatory obligations and applied.
2. Handle and sort concrete materials and components.	2.1. On delivery to site, concrete materials and components are identified and checked for conformity to material schedule, plans and specifications. 2.2. Concrete materials are moved to specified location applying safe manual handling procedures. 2.3. Concrete materials and components are stacked or stockpiled for ease of identification and retrieval for task sequence and job location in accordance with job specifications. 2.4. Concrete materials and components are protected against physical and water damage and stored clear of access ways, for ease of identification, retrieval and distribution. 2.5. Components are handled and positioned ready for installation in accordance with manufacturer recommendations, plans and specifications.
3. Handle and remove concrete materials and components on completion.	3.1. Materials are handled safely according to MSDS and requirements of regulatory authorities. 3.2. Hazardous material is identified for separate handling. 3.3. Dust suppression procedures are used to minimise health risk to work personnel and others. 3.4. Protection of materials is provided in accordance with specific material needs. 3.5. Materials are stored safely and effectively according to MSDS and requirements of statutory and regulatory authorities.
4. Clean up.	4.1. Work area is cleared and materials disposed of, reused or recycled in accordance with legislation, regulations, codes of practice and job specification. 4.2. Hazardous material is identified for separate handling. 4.3. Non-toxic materials are removed using correct procedures. 4.4. Dust suppression procedures are used to minimise health risk to work personnel and others. 4.5. Tools and equipment are cleaned, checked, maintained and stored in accordance with manufacturer recommendations and standard work practices.

Required Skills and Knowledge

REQUIRED SKILLS AND KNOWLEDGE
This section describes the skills and knowledge required for this unit.
Required skills
Required skills for this unit are: communication skills to: determine requirements enable clear and direct communication, using questioning to identify and confirm requirements, share information, listen and understand follow instructions read and interpret: documentation from a variety of sources drawings and specifications report faults use language and concepts appropriate to cultural differences use and interpret non-verbal communication, such as hand signals evaluating own actions and making judgments about performance and necessary improvements identifying and accurately reporting to appropriate personnel any faults in tools, equipment or materials organisational skills, including the ability to plan and set out work recognising procedures, following instructions, responding to change and contributing to workplace responsibilities, such as current work site environmental and sustainability frameworks or management systems teamwork skills to coordinate own work with others to action tasks and relate to people from a range of cultural and ethnic backgrounds and with varying physical and mental abilities technological skills to: use a range of mobile technology, such as two-way radio and mobile phones voice and hand signals to access and understand site-specific instructions.
Required knowledge
Required knowledge for this unit is: concrete materials handling techniques concreting materials general construction terminology hazardous materials job safety analysis (JSA) and safe work method statements MSDS materials storage and environmentally friendly waste management plans, drawings and specifications processes for the calculation of material requirements quality requirements types, characteristics, uses and limitations of tools and equipment workplace and equipment safety requirements.

Evidence Guide

EVIDENCE GUIDE
The evidence guide provides advice on assessment and must be read in conjunction with the performance criteria, required skills and knowledge, range statement and the Assessment Guidelines for the Training Package.
Overview of assessment	This unit of competency could be assessed in the workplace or a close simulation of the workplace environment, provided that simulated or project-based assessment techniques fully replicate construction workplace conditions, materials, activities, responsibilities and procedures.
Critical aspects for assessment and evidence required to demonstrate competency in this unit	A person who demonstrates competency in this unit must be able to provide evidence of the ability to: locate, interpret and apply relevant information, standards and specifications comply with site safety plan and OHS legislation, regulations and codes of practice applicable to workplace operations comply with organisational policies and procedures including quality requirements safely and effectively operate and use tools, plant and equipment communicate and work effectively and safely with others safely handle the materials and components in the mandatory tasks.
Context of and specific resources for assessment	This competency is to be assessed using standard and authorised work practices, safety requirements and environmental constraints. Assessment of essential underpinning knowledge will usually be conducted in an off-site context. Assessment is to comply with relevant regulatory or Australian standards' requirements. Resource implications for assessment include: an induction procedure and requirement realistic tasks or simulated tasks covering the mandatory task requirements relevant specifications and work instructions tools and equipment appropriate to applying safe work practices support materials appropriate to activity workplace instructions relating to safe work practices and addressing hazards and emergencies material safety data sheets research resources, including industry related systems information. Reasonable adjustments for people with disabilities must be made to assessment processes where required. This could include access to modified equipment and other physical resources, and the provision of appropriate assessment support.
Method of assessment	Assessment methods must: satisfy the endorsed Assessment Guidelines of the Construction, Plumbing and Services Training Package include direct observation of tasks in real or simulated work conditions, with questioning to confirm the ability to consistently identify and correctly interpret the essential underpinning knowledge required for practical application reinforce the integration of employability skills with workplace tasks and job roles confirm that competency is verified and able to be transferred to other circumstances and environments. Validity and sufficiency of evidence requires that: competency will need to be demonstrated over a period of time reflecting the scope of the role and the practical requirements of the workplace where the assessment is part of a structured learning experience the evidence collected must relate to a number of performances assessed at different points in time and separated by further learning and practice, with a decision on competency only taken at the point when the assessor has complete confidence in the person's demonstrated ability and applied knowledge all assessment that is part of a structured learning experience must include a combination of direct, indirect and supplementary evidence. Assessment processes and techniques should as far as is practical take into account the language, literacy and numeracy capacity of the candidate in relation to the competency being assessed. Supplementary evidence of competency may be obtained from relevant authenticated documentation from third parties, such as existing supervisors, team leaders or specialist training staff.

Range Statement

RANGE STATEMENT
The range statement relates to the unit of competency as a whole. It allows for different work environments and situations that may affect performance. Bold italicised wording, if used in the performance criteria, is detailed below. Essential operating conditions that may be present with training and assessment (depending on the work situation, needs of the candidate, accessibility of the item, and local industry and regional contexts) may also be included.
Information includes:	diagrams or sketches instructions issued by authorised organisational or external personnel manufacturer specifications and instructions, where specified MSDS memos regulatory and legislative requirements pertaining to handling concreting materials relevant Australian standards safe work procedures relating to handling concreting materials signage verbal, written and graphical instructions work bulletins work schedules, plans and specifications.
Planning and preparation include:	assessment of conditions and hazards determination of work requirements and safety plans and policies equipment defect identification work site inspection.
Safety (OHS) is to be in accordance with state and territory legislation and regulations and project safety plan and may include:	emergency procedures, including extinguishing fires, organisational first aid requirements and evacuation handling activities that may require the assistance of others or the use of manual or mechanical lifting devices where size, weight or other issues, such as a disability are a factor hazard control hazardous materials and substances, including cement and curing agents organisational first aid PPE prescribed under legislation, regulations and workplace policies and practices safe operating procedures, including the conduct of operational risk assessment and treatments associated with: earth leakage boxes lighting power cables, including overhead service trays, cables and conduits restricted access barriers surrounding structures traffic control trip hazards work site visitors and the public working at heights working in confined spaces working in proximity to others use of firefighting equipment use of tools and equipment workplace environmental requirements and safety.
Tools and equipment include:	brooms rakes shovels tarpaulins and covers wheelbarrows.
Quality requirements include relevant regulations, including:	Australian standards internal company quality policy and standards manufacturer specifications workplace operations and procedures.
Materials:	include: aggregates cement form release agents non-toxic materials, including general concreting materials sand water may include: additives curing compound oxides.
Environmental requirements includes:	clean-up management dust and noise dust suppression, including: covering keeping dust in the air to a minimum spraying with water using a vacuum cleaner stormwater management vibration waste management.
Concrete materials and components:	include: bar chairs bracing plastic membrane reinforcement mesh spacers steel and timber formwork may include: bar steel decking key joints push-pull props reinforcement bars scaffolding support props tilt panels.
Handling procedures include:	calculation of quantities manual handling, including: carrying materials using correct lifting techniques control of waste using pallets MSDS protection of materials stacking and storing of materials.
Statutory and regulatory authorities include:	federal, state and local authorities administering the applicable Acts, regulations and codes of practice.

Unit Sector(s)

Unit sector	Construction

Co-requisite units

Co-requisite units	Nil

Functional area

Functional area